IPX-2000 FW 140567 Release Note

Please unpack the file you'll get two firmware files. 

Firmware upgrade instruction

NOTE: 

If currently installed version is a 1.5 release and a downgrade to this 1.4 version is expected, please upgrade HF_TX_GE_to14 package (E2K_xxA_HF_TX_GE_to14-1144939242.bin)at first. After upgrading this HF package GUI will respond Upgrade Failed, please ignore that as it is just a work-around to prevent system from rebooting.

 
Be sure to update the firmware files in correct sequence (login machine via web browser HTTPs session and find the PBX firmware in the system menu to complete the firmware upgrade):


1. Back up current configuration

2. Upgrade BR package to advance boot loader (IPX-2000 only): E2K_xxA_BR_TX_GE_20060321-1145006652.bin

Please wait for few minutes till machine finishes loading firmware and rebooting. After machine rebooting, there will be prompt window about machine reboot completed. At this moment, press the OK button of the prompt window, no need to close the existing firmware upgrade window, continue loading the firmware step 3:


3. Upgrade OE package to advance OS to version 1.0.27: E2K_xxA_OE_TX_GE_1027-1151393182.bin 

Please wait for few minutes till machine finishes loading firmware and rebooting. After machine rebooting, there will be prompt window about machine reboot completed. At this moment, press the OK button of the prompt window, no need to close the existing firmware upgrade window, continue loading the firmware step 4:


4. Upgrade KN package to advance kernel image: E2K_xxA_KN_TX_GE_20060324-1143180164.bin

Please wait for few minutes till machine finishes loading firmware and rebooting. After machine rebooting, there will be prompt window about machine reboot completed. At this moment, press the OK button of the prompt window, no need to close the existing firmware upgrade window, continue loading the firmware step 5:


5. Upgrade HF_TX_GE_allowmbin package to allow .mbin package upgrade later: E2K_xxA_HF_TX_GE_allowmbin-1144688476.bin

Note that GUI will respond Upgrade Failed, please ignore that and continue loading the firmware step 6.


6. Upgrade AP (.mbin) package to advance to current version: E2K_01A_AP_TX_PL_140567.mbin

After loading the firmware files, it is suggested to load the factory default settings to activate the new configurations. Power off the machine, press the RESET button on the front panel; power on machine, and wait 3-5 minutes till machine configurations are fully loaded for evaluations.


Support_VoIP@planet.com.tw