Thanks for purchasing PLANET FGSW-2620VMP4 Layer 2 Management Ethernet Switch.
This document provides the firmware release note and history of the product

Version 1.23 Released at 2012/01/30

Firmware version: 1.23
Release at 2012/01/30

This firmware provides the following modification:

A. Bug Fixed -

1. Change PoE mode name from Priority to Classification.
2. Fix the Switch offering class 3 devcie to 16Watts PoE power budget.
3. Fix port1 can't receive IGMP query control packet issue.
 

B. Function Added -

1. SMTP Alarm.
2. Per port Remote ping.
3. Users configuration. It offers 3 permissions which Admin, Operator and Viewer.
   Admin: Full control to the switch.
   Operator: Full control to PoE configuration only.
   Viewer: Read only.   
  
4. Backup configuration without IP address.
5. Port description.
6. Move and add Rate Limit web page.
7. Add PoE mode of consumption. (Default value, it offers PoE power to the PD according to real power consumption.)
8. Add PoE Admin function.
9. Add system log.

[Upgrade Requirements]:

1. The latest firmware version of FGSW-2620VMP4
2. The FGSW-2620VMP4 switch
3. Workstation with Microsoft IE 6.0 or above.
4. TFTP server. (If you want to upgrade firmware via TFTP)


[Upgrade procedure]:

1. Connect the RJ-45 UTP cable to the target switch.

2. Login is required to access the WEB interface after the switch boot completes successfully. The factory default user name and password is "admin".

3. After Web main screen appeared, click the "System --> Firmware Upgrade" at the left Menu.  

4. The screen provided HTTP Firmware Upgrade and TFTP Firmware Upgrade.

   A. HTTP Firmware Upgrade
     (1) Enter the "Browse.." button to locate firmware path.
     (2) Click "Submit" button to start the firmware upgrade procedure.Please don't power off the switch while procedure be started.
     (3) Please wait until the system reboot complete.
     (4) Reset to factory default again.

   B.TFTP Firmware Upgared

     (1) Enter the "TFTP Server IP Address" and filename with the correct firmware file.
     (2) Click "Apply" button to start the firmware upgrade procedure. Please don't power off the switch while procedure be started.
     (3) Please wait until the successful message shows in the Update Status web page.
     (4) Please wait until the system reboot complete.
     (5) Reset to factory default again.

5. Relogin the switch via WEB browser. Please click the "System -->System Information --> Firmware Version" to double check if the firmware be upgraded successfully.
 

*************************
Firmware Release History:  
*************************

Firmware version: 1.22
Release at 2010/05/12 

This firmware provides the following modification:

A. Bug Fixed - 

1. Fix PoE unit temperature shows wrong. 


B. Function Added - N/A

*****************************************************
Firmware version: 1.20
Release at 2010/02/10 

This firmware provides the following modification:

This is initial version.

A. Bug Fixed - N/A 

B. Function Added - N/A


Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw


