PLANET Network Video Recorder Firmware Release
----------------------------------------------
Product support: NVR-3250 
Release Date:    2012/08/16 
Release Version: 2.2.1.52225
Previous Release: 2.1.1.50311

Added
-PTZ Panel in web UI will gray out if PTZ is not supported.
-Add new log messages:
¡§Settings of user account have been modified"  
¡§Settings of user group have been modified¡¨  
¡§System time has been changed¡¨ 
-Add IE environment test tool (When system detects that ActiveX cannot function properly, it will pop-up download IE environment tool message.)
-Web UI Channel Status page will show info of recording stream
-Add Lithuanian version web UI
-Add new log messages for USB backup (Start/End, Time, Channel ID)
-Cannot detect camera from different clients at the same time
-Export AVI to USB Storage function
-UPS support
-ONVIF support (ONVIF Test Tool v1.02.2.10)
-Configurable file name for event image
-Playback display millisecond for single step on web UI
-Boot screen
-Modify web UI default font to Verdana for German, Danish, Czech, Polish, FRENCH, Russian, Slovakian, Hungarian, Korean, Turkish, Finnish, Dutch
-Full screen lock (VGA Output)
-Auto login (VGA Output)
-Preset sequence dwell time (VGA Output)
-USB Joystick Support (VGA Output)

Modified
-Change system log from ¡§Stop recycling HDD space¡¨ to ¡§Cleaning HDD space process finished¡¨
-Only write system log when recycle size is not zero and recycle is finished
-Web UI "Setup" menu tree "+", "-" icons no action
-Pre-alarm time increases to 60 seconds
-UPnP port forwarding self check mechanism to prevent failed message even after port has been successfully configured
-Error message when users set DHCP assignment exceeds available IPs
-Limit the amount of DHCP Client to 50
-Add new web message when leaving Auto setup page: ¡§Terminating process, please wait¡K¡¨ 
-When the Auto Setup function is not supported, even camera list is blank, it will not direct to Auto Setup web page.
-Web page will be closed if server does not response while performing Auto Setup
-Local UI system Log display will sync with web UI.

Fixed
-Server crashes if recorded data is invalid
-Fixed the issue that if the Export/Playback time is close to current¡@system time, the recording data may be false.
-Fix data error will occur while fast forwarding if playback data time is close to current system time.
-After clicking enter in Google map setup page, no need to refresh the page.
-While testing SMTP, if user does not check test checkbox, ID and password will not be sent.
-After setting FTP server, send message function in general setting section will be enabled automatically.
-Unable to cancel while detecting camera
-Fixed the error message ¡§Error retrieving recording data¡¨ to ¡§Export complete ¡§if user set AVI/JPEG export end time in future.
-When all channels are added with cameras, the search table in camera setting page should be empty.
-While preset SEQ List is empty, Preset SEQ button should be disabled.
-If NVR has DO, the table title of DI/DO setting should be DI/DO setting
-When adding new cameras, system will remove the unacceptable characters in model name or device name first, and then display the remaining words in camera name field. (Web)
-Can not disable audio recording when alarm length is not zero
-Can not export to AVI from web anymore if export to future time first
-Error message when incorrect encoding is used in preset name
-PTZ speed cannot use normally on some cameras
-PTZ panel on web UI does not work for Panasonic SW395
-Unable to change recording stream format in web UI
-(Web) If user checks any items at Event Trigger section, both Send Message and Enable Authentication items will be checked automatically.
-Event cannot function properly if user remove camera from one channel and then add a new camera in the same channel.
-Event after auto setup is done, the last camera in search result list still shows detecting.
-After adding camera by auto setup once, if user performs auto setup function again in web UI, all camera will be deemed "Incompatible"
-Fixed the inconsistency of resolution option of AXIS P3301 under ONVIF mode and web.
-Unable to change ONVIF camera setting
-Fixed the issue that while performing playback in VGA Output UI, user must click search twice to get video data.
-When both user playback recording data in both VGA Output UI and web UI simultaneously, web UI will show "Permission Denied" message and user cannot log in.
-After restore NVR's setting, the resolution will become blank if user changes the format in Recording Frame Rate section from web UI.
-PTZ Panel on web UI does not work for Panasonic SW395

Note
-The whole of update time need about two minutes
-Performed update need do reset to default


=======================
*** NVR-3250 _2.1.1.50311
Product support: NVR-3250 
Release Date:    2012/06/27 
Release Version: 2.1.1.50311
Previous Release:  N/A

*** NVR-3250 _2.1.1.50311
a) Initial release version


Firmware upgrade process
========================
Please don¡¦t decompress firmware file (*.tar.gz).
Before upgrade the NVR firmware, please disable your Anti-Virus software first.
(because some anti-virus software will block the upgrade process)
And follow steps as below to upgrade NVR-3250's firmware¡G
 Step1. Go to ¡§NVR Setup¡¨ page first.
 Step2. Go to ¡§System Options¡÷Maintenance¡¨ page.
 Step3. Find the ¡§Upgrade NVR Firmware¡¨ at the right side of page.
 Step4,5. Press ¡§Browse¡¨ button and select the Firmware(*.tar.gz) 
 Stpe6. Press ¡§Upgrade¡¨ button to apply upgrade your NVR.
After upgrade, we strong recomand to reset the NVR as default.
It will make the device work more stable.

Note:
=====
Do not turn the power off during the upgrade process. This will damage the unit.
This firmware is for NVR-3250 only, and please reset the device to the factory default setting after the upgrading.

Thanks for choosing PLANET products, any comment or feedback will be appreciated.

Best Regards,
PLANET Tech Support Team
Technical support:support@planet.com.tw